

**Preisträger 2022 Kategorie** **Produkt**

**X-Change Technologie**  
Molto Luce GmbH

Die Molto Luce X-Change Technologie ermöglicht den einfachen Wechsel einer LED-Platine, ohne die gesamte Leuchte tauschen zu müssen. Der Wechsel erfolgt mittels Bajonette-Verschluss und funktioniert komplett werkzeuglos. Bei einem Defekt, einer Anpassung an effizientere Komponenten oder Änderungen der Lichtfarbe, Lichtstrom oder CRI-Werte, muss nicht mehr die gesamte Leuchte getauscht werden, sondern nur das serienfertige Chip-on-Bord-LED-Modul. Dies führt zu weniger Materialverschwendung sowie einem geringeren Transportaufwand.

Bild: © IDZ | Molto Luce GmbH

**Award winner 2022 Product Category**

**X-Change Technology**

Molto Luce GmbH

Molto Luce X-Change technology enables the straightforward replacement of an LED circuit board without the necessary replacement of the entire lighting fixture. The task is carried out by means of a bayonet connection and is entirely without tools. In the event of a defect, modification to more efficient components or changes in light colour, luminous flux or CRI values, it is no longer necessary to replace the entire luminaire, but only the production-ready chip-on-board LED module. This results in reduced material waste as well as transport effort and expense.

Photo: © IDZ | Molto Luce GmbH